

|  |  |  |  |
| --- | --- | --- | --- |
| Customer |  | Date |  |
| Unit Model |  | Unit Serial No. |  |

CHECKS PERFORMED

|  |  |  |
| --- | --- | --- |
| **Description** | **Pass** | **Fail** |
| Solar Panels - Check for any visible damage (cracks scratches etc.) |  |  |
| Solar Panels - Ensure mounting brackets are functional and secured to canopy. |  |  |
| Batteries - Inspect for leaks, corrosion and proper terminal connections. |  |  |
| Batteries - Verify that the batteries are securely mounted. |  |  |
| Inverter - Inspect for any physical damage or loose parts. |  |  |
| MPPT Charge Controllers - Verify that all connections are tight and correctly labeled. |  |  |
| Canopy - Inspect the enclosure for integrity and damage. |  |  |
| Cooling System - Check cooling fans for cleanliness. |  |  |
| Cooling System – Check filters are clean on canopy vents |  |  |
| Inverter - Test AC output voltage and frequency |  |  |

**Comments**

|  |  |  |
| --- | --- | --- |
| Name | Signature | Date |
|  |  |  |